PICP AR

Printer Port FSK Modem

Hardware Documentation BayCom

–2–

Important Notice:

All texts, listings, diagrams, drawings, sketches and circuits in this manual are

copyright protected. Any publication or distribution of the manual or parts

thereof require the prior permission of the authors. The assembly of the

electronic circuitry described in this manual for other than strictly private

purposes is not permitted. In particular, it is prohibited to use the design

commercially . Offenders will be prosecuted.

The authors accept no liability for the correctness of the circuits published or

their technical documentation. They are also not to be held liable for damages

that may occur as a result of the construction or operation of the circuits

described, the corresponding kitset or the fully built–up unit.

The copyright for the modem is held by Wolf–Henning Rech, DF9IC and

Johannes Kneip, DG3RBU. The copyright holder ’ s contact address is

BayCom GmbH

Massinger Weg 3

93107 Weillohe

GERMANY

–3–

PICP AR – a simple printer port FSK–Modem

Not too complicate and cost sensitive equipment are the basic preconditions, when

a new a amateur radio operation mode is predetermined to gain a lot of friends. With

the advent of simple interface modem equipment for 1200Bd AFSK at the end of the

eighties, packet radio gained lots of popularity. A steadily increasing number of users

and huge amounts of data called for higher transmission rates. The FSK data

transmission standard, designed by James Miller, G3RUH ten years ago, soon

became a world wide standard. But it still did not succeed to drive out the old

fashioned slow AFSK modes.

The reasons were twofold: To get started with 9600Bd, at least a PC slotcard or a TNC

instead of a simple modem was required. Also, there were only few radios suitable

for 9600Bd, modifications often proved difficult. Unfortunately, the last has not yet

changed. On the modem sector, the BayCom PAR96 first brought some life into the

house: This was a simple FSK modem, directly connected to the PC’s printer port and

much cheaper than a TNC. To reduce the interrupt load on the PC, this modem

featured an internal FIFO, transmitting 16 bit collected in single serial bursts from and

to the modem. Per burst one interrupt was required, thus reducing the thrilling 9600

interrupts per second to as less as 600 interrupts per second, half of the rate required

for the old 1200Bd AFSK modems. Scrambling of the data and the DCD were

performed by the PC. All other functions like filtering, clock regeneration and data

reconstruction were implemented in the modem, using standard CMOS ICs and low

density programmable devices like GALs and EPROMs. This resulted in a modem

half the size of a standard euro PCB (80*100mm) and a power consumption of about

160mA@5V .

The new PICPAR modem presented here is a successor of the PAR96. Our intention

was to design a low–power, low–cost version of this modem, especially to abandon

the need for an external power supply. But it should be compatible with the PAR96

to conserve all the precious software work done for the PAR96 drivers.

The highest cost in the original PAR96 design was the digital FIR filter, the FIFO

control and the clock regeneration. Here an idea raised to integrate these functions

into a small low cost microcontroller. Our choice was the PIC16C84 by Microchip.

This is a full 8 bit microprocessor in an 18 bit DIL housing. It offers 13 I/O ports, 36

byte RAM, 1k EEPROM an integrated oscillator and a lot of other bells and whistles,

making it an ideal device for this purpose. This processor also starts operation at 2

volts and requires only 2mA supply current at 4 MHz clock, making it a good starter

for an interface powered modem with only 3–5mA total power consumption.

Modem schematics

The figure on the next page shows a block diagram of the modem. The printer

interface connection is realized with 6 wires. An excellent DCD could also be

integrated into the PIC, thus utilizing the already specified, but not yet used DCD line

on the PAR96 interface. The modem provides an interrupt clock with a 16 times

RX–/TX clock period. Within the next half clock period, the PC is expected either to

–4– clock 16 new transmission bits into the modem or to empty the FIFO containg 16 bit

newly received bits.

Printer port

Data – FIFO

Analog

low pass

Analog

low pass

PTT

TXD

BURST

RXD

CLK/16

T o

modulator

From

demodulator

DCD

PICP AR–Modem

D/A–

converter

PC

PIC 16C84

FIR–Filter

DCD

Clock recovery

Data reconstruction

Both is realized via a burst clock generated by the PC. The PIC performes the

transmitter FIR filter an the incoming data and passes the result to a 7 bit D/A

converter . On the receiver branch, a lot more functions have to be carried out: First,

a clock signal has to be recovered from incoming data. Then data have to be

reconstructed and a carrier detection has to be performed. The regenerated data are

fed into a FIFO, from where they are handed over to the PC.

Besides PIC and FIFO some analog functions are required. The raw signal from the

D/A–converter has to be smoothed by an analog low pass filter, passing the data via

a deviation control to the radio modulator. Incoming data first pass an anti–aliasing

filter , before they are digitalized by a comparator stage and fed into the PIC processor.

Schematics

The modem schematics on this manual’s center page mirrors the block diagram. For

an efficient practical realization some tricks were required which are explained in this

section. The power supply for the modem is gained from the output ports of the

centronics interface via the Schottky diodes D1–D3. Typically an operating voltage

of 4.5V can be gained, even from laptops, but the circuit already operates from 3V

and up. Stabilization is not required, C1 and C5 are used to smooth the power supply.

The FIFO utilizes a CMOS 4517 circuit. This is a 64 bit shift register with an auxiliary

output at 16 bit. Clock lines are shared by PIC and PC. When the PIC switches it’s

output into high impedance, the PC becomes clock master.

R22 and C2 generate a reset signal for the PIC processor, which operates on a 3.686

MHz clock. T1 inverts the low active PTT, T2 switches the radio PTT. A MOS transistor

is used to achieve proper switching at low gate current.

T o minimze power consumption, we use a R–2R resistor network as DA–converter

instead of an integrated solution (R5–R11). 1% tolerance metal film resistors are

mandatory to achieve a proper output signal.

–5–

The following active filter and amplifier net is already well known from similar modem

implementations. We utilize a 4–way integrated amplifier OP491. This type is a bit

more expensive than the usual bulk OP’s, but it shows low power consumption,

rail–to–rail–operation to achieve a maximum of deviation. It’s low tendency for

oscillations saves external load resistors, again reducing power consumption. Just

one simple 1k–Ohm load would just double the modem’s supply current!

For the receiver, the OP can also be used as a comparator (IC3D). To gain the

reference voltage for the input signal sampling we use the first stage of the transmitter

filter together with a software generated suitable output of the D/A converter.

The modem output is DC decoupled via C9. All radio signals are led to a 9p. D–Sub

connector .

Assembly

The whole modem is assembled on a double sided PCB of size 30 * 72mm (see

below). There are only a few feed throughs to connect if you should use a home–brew

PCB. The assembly itself is fairly uncritical. At first all the lower passive components

are placed and soldered. Then all other passive and active components are

assembled and soldered. Do not yet solder the connectors. For the ICs, precision

sockets should be used. When the assembly is finished, check the board for bad

solderings or short circuits. Finally, the three ICs are inserted into their sockets, take

care for correct orientation.

–6–

–7–

Part List:

R1 4k7 C7 100p ceramics 2,54 ls

R2 100k C8 1n ceramics 2,54 ls

R3 47k C9 10u, 6.3V tantalum, 2,54 ls

R4 100k C10 100n Folie, 5,08 ls

R5 1.30M* C1 1 1n ceramics, 2,54 ls

R6 649k* C12 220p ceramics, 2,54 ls

R7 324k* C13 100n, 5,08 ls

R8 162k* C14 1n ceramics, 2,54ls

R9 80.6k* C15 100n, 5,08 ls

R10 40.2k* D1 BA T43

R1 1 20.0k* D2 BA T43

R12 100k D3 BA T43

R13 56k

R14 12k T1 BC548 or equivalent

R15 10k trimmer T2 BS107 or equivalent

R16 2k2

R17 100k IC1 PIC16C84, programmed

R18 82k IC2 OP491

R19 39k IC3 CD4517

R20 27k

R21 27k St1 Sub–D 25p., male

R22 47k St2 Sub–D 9p., male

C1 100uF , 10V electrolyt, 2,54ls

C2 10u, 6.3V tantalum, 2,54ls F1 IC–socket, 18p.

C3 27pF ceramics 2,54 ls F2 IC–socket, 16p.

C4 27pF ceramics 2,54 ls F3 IC–socket, 14p.

C5 3n3 ceramics 2,54 ls

C6 470p ceramics 2,54 ls Q1 Crystal 3.686 MHz

PCB PICPAR

Case AGM25

Resistors marked with *: 1% tolerance (E96), all others: 5% tolerance

ls means ”lead space”

–8–

Mounting the case

The size of the PCB was dimensioned for a small plastic case (AGM25, available from

several distributors). This compact housing is dedicated for PCBs carrying Sub–D

connectors, carrying the board. The connectors are fixed between both halfes of the

case.

T o achieve a proper fitting into the case, both sub–D connectors are slipped onto the

board pads, but not yet soldered. Then the PCB is put into one of the case halfes and

the connectors are adjusted to match the required distance. Then all connector pads

are soldered properly. On the upper half of the case, a 4mm hole can be drilled to

allow access to the deviation adjustment trimmer.

Connecting computer and radio radio

St 1 of the modem is directly connected to the printer port of your computer. Plug the

modem direclty onto your DB–25 interface or use a shielded 1:1 cable as short as

possible.

All leads required to connect the radio to the modem are available on a 9–pin sub–D

male socket on the modem. Only four lines need to be connected: Audio to transmitter

(TX–AF), audio to receiver (RX–AF), PTT and ground.

The transmitting signal is fed directly into the radio’s modulator. The PTT is active low,

i.e., it switches to GND during transmission. The received signal is taken directly from

the demodulator. At this stage it is appropriate to mention that most radios must be

converted for 9600Bd operation. So far, only very few radios are available

commercially that allow for the direct connection of 9600 Bd FSK modems such as

this one. However, some of the major manufacturers have recently presented radios

that feature a 9600Bd packet connector. When choosing a radio, please keep in mind

that the switching times for 9600Bd signals on most synthesizer radios are very long

and will hence affect your throughput as you will require a rather long TXDELAY .

Whenever possible, a crystal controlled radio should be used, such as, e.g., the TEKK

KS–960.

1 5

6 9

6–9 = Ground

1=TX–AF 3=PTT 5=RX–AF

–9–

Getting started

The PICPAR modem can be used with all drivers that were designed for the BayCom

P AR96 modem. The BayCom L2–driver (from version 1.60) is one possible

alternative, the TFXPAR driver by DB7KG for the use with hostmode programs is

another one. Drivers are also included in the latest UNIX kernels and in

PC–FLEXNET . A first functional check of the modem should be done using the

BayCom L2 driver. Start INSTALL and select the ”PAR96” when prompted for the

hardware on the corresponding interface. Start L2. If an error message should be

prompted, start L2.EXE again. Because the first start of L2 switches on the modem’s

power supply, the modem might not react fast enough. Other drivers might behave

similarly . When L2.EXE responds with a flashing rectangle in the upper right screen

corner , the modem is working properly and generates regular data interrupts (even

when no radio is connected). After starting the BayCom terminal SCC.EXE and

connecting the radio, it should be possible to monitor the channel.

One difference between the PICPAR and the old PAR96 modem is that it provides a

proper hardware DCD. This should be considered when setting the MODE

command. This parameter is configured to :MODE 9600c by default (software DCD).

With the PICPAR modem, it should be set to :MODE 9600. Then the modem’s

hardware DCD is used.

As the only adjustment, the deviation has to be set properly. R15, accessible on the

top of the modem should be set to the correct output level for your radio. Either refer

to your radio manual or try to find the correct deviation (+/– 3 kHz) by trying. At this

deviation, the noise generated when a packet is transmitted (set high TXDELAY for

better observability) should match the noise to be heard in your radio on an unused

channel at opened squelch. If there should be retries during your practical work with

your modem, try to optimize the adjustment of R15. Please note again, that you need

a special radio prepared for 9600Bd or a proper modified radio to achieve good

transmission quality for 9600Bd FSK. Especially switching times, PLL behaviour and

AF bandwidth are important factors, which might corrupt your signal when your radio

does not meet the 9600Bd requirements.

–10–

T roubleshooting

The modem assembly is pretty simple, there are no critcal parts. Possible assmbly

errors should be easy to localize. If L2 does not recognize the modem (error message

after starting L2.EXE) check the modem’s power supply first. The voltage between

pin 8 and 16 of IC2 should range between 3 and 5 V after first start of L2.EXE. After

powering up the modem, is there a correct RESET at pin 4 of the modem (voltage

should rise to supply voltage shortly after powering up). Does the crystal oscillate?

If the modem responds, but the PTT does not switch, a wrong assembly of T1 or T2

might be the reason. If there is no transmission or receiving, first check the path

between R12 and the output of the modem on the transmitter branch with an

oscilloscope. On the receiver branch, check the signal between the modem input to

pin 14 of the OP491. In most cases a short circuit or a bad soldering will eliminate the

analogue signal. If your centronics connector should have very low impedance

pullups on the PE input line (we use it for data receiving) the shift register output might

be overloaded. In this case a small driver (inverting or non inverting) beween pin 1

of the 4517 shift register and pin 12 of the centronics connector might cure the

problem.

Further recommendations

Usually , the modem can be put directly onto the centronics port. If you use a printer

cable, it should be as short as possible and shielded. Also the radio cable should be

properly shielded and as short as possible. The shield should always be connected

to ground only on one side of the cable. A proper grounding with an extra cable

between PC and radio improves signal quality and reduces damage in case of a

lightning strike into your antenna. The modem itself is only designed for half duplex

operation, full duplex operation with concurrent transmission and receiving is not

possible.

Drivers for the modem exist not only in the BayCom software. The program TFXPAR

by DB7KG operates the modem together with any hostmode programs. A driver is

also included in the most recent Linux kernels, written by HB9JNX. BayCom itself is

a DOS application, but on most computers an operation under Windows 3.x should

be possible by first loading the L2.EXE driver and then starting windows. The terminal

itself then can be operated in any DOS window.

Enjoy the assembly and the use of the PICPAR modem!

Y our BayCom team.

–1 1–

BayCom

BayCom ordering information

Ordering of BayCom Hard– and Software

Y ou can order all BayCom products directly from the BayCom–team, address see below.

Please ask for our catalogue and price information.

BayCom products can also be obtained by authorized dealers all over the world.

Order Information:

8500 PICP AR, kit with standard components, including case

8600 PICP AR, assembled, in case

8601 PICP AR, PCB +programmed PIC–processor

T echnical Support and Service

For all BayCom kits we offer a repairing service. Surely you will understand, that this service

cannot be provided for free, but we will try to do it as cheap as possible. We know about the

amateurs need having assembled a kit that does not work! Note that we are a part time ”just

for fun” company and cannot provide any 24 hour services or telephon hotlines. If you have

a question, send us a FAX or send an e–mail to baycom@baycom.de

If there is a major damage (more than half of the kit price) we will ask you before we do the

repair . Please send all equipment for repair to the following address:

BayCom GmbH

Johannes Kneip (DG3RBU) T el. ++49 5105 585050

Bert–Brecht–W eg 28 F AX ++49 5105 585060

30890 Barsinghausen

GERMANY

Y ou also can get technical information from Johannes!

BayCom

BayCom Hard– und Software GmbH

Massinger Weg 3

D–93107 Weillohe

T el. 09453/9819

F AX 09453/9829